{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["template"],"not_rendered":{"charts":1,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"template","index":0,"n_rows":55,"n_cols":7,"rows_kept":55,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["Plan"]
["Year"]
["Reference"]
["Input Materials","mass (g)","renewable source ?","mass renewable source (g)",null,"energy mix"]
["Reagents",{"$nulls":4},"nuclear",0.584]
[{"$nulls":5},"natural gas",0.062]
[{"$nulls":5},"unaccounted",0.008]
[{"$nulls":5},"non-renewables",0.6539999999999999]
[{"$nulls":5},"hydro",0.239]
["Reaction Solvents",{"$nulls":4},"wind",0.08]
[{"$nulls":5},"solar",0.023]
[{"$nulls":5},"bioenergy",0.005]
[{"$nulls":5},"renewables",0.34700000000000003]
["Catalysts",{"$nulls":4},"total",1.001]
[]
[]
["Workup"]
[]
[]
[]
[]
["Purification"]
[]
[]
[]
[]
["SUM",0,null,0]
[]
["Product","mass (g)"]
["vanillin",1000]
[]
["Waste Products","mass (g)","reusable ?","mass reusable waste (g)"]
{"$rows_empty":10}
["SUM",0,null,0]
[]
[]
["mass renewable inputs",0,"g"]
["mass reusable waste",0,"g"]
[]
[null,"Actual","Sustainable Limit"]
["F(VI)",{"$error":"#DIV/0!"},1]
["F(VO)",{"$error":"#DIV/0!"},1]
["F(RE)",0,1]
["F(VP)",0.7,1]
[]
["sustainability index",{"$error":"#DIV/0!"}]