CONFIGURATION INFORMATION
=========================

Path         : C:/Bruker/TopSpin3.2/conf/instr/spect/uxnmr.info
Date         : Thu Aug 10 12:34:00 2023
Release      : TOPSPIN Version 3.2-pl6
Installed in : C:/Bruker/TopSpin3.2
Host         : CAPSL72218
OS           : Windows 7 (Vs 6.1) Service Pack 1
CPU          : Intel(R) Core(TM) i7-4770 CPU @ 3.40GHz (8 cores at 3392 MHz with Hyperthreading)
User         : ISD\nmruser
Description  : Avance III 600
Location     : 
System       : Avance III NMR spectrometer
1H-frequency : 600.13 MHz
Order Number : 
Configured in: C:/Bruker/TopSpin3.2/conf/instr/spect

IPSO: connected to spectrometer subnet
- TCP/IP address = 149.236.99.249
- Tctrl : 1
- Fctrls: 3
- Gctrl1: without digital preemphasis
- Rctrl : none
- FREDs : none
- DPP : none

DRU: AQS DRU-E Z102520/00539 ECL 03.00
- TCP/IP address = 149.236.99.89
- Firmware Version = 131205
- DRU controls AQS-Rack and HPPR/2

AQS: connected to 149.236.99.89:/dev/tty10
  _Slot_ SBSB _____________________Board_____________________
  Number Addr Type HW-VS FW-VS ID  ECL Name   Description
  -----------------------------------------------------------
     2   0x10 0x42   0x3    AW  R  3.0 REC-1  AQS RXAD600 Z102117/272 ECL 03.00
     3   0x34 0xc0   0x1        X  1.0 REF-1  REF-600 Reference Board for AQS Receiver
     4   0x24 0x19   0x8    AE  S  2.0 SGU-1  AQS SGU/2 600 Z103081/00171 ECL 02.00 FPGA-Vs=AF
     5   0x25 0x19   0x8    AE  S  2.0 SGU-2  AQS SGU/2 600 Z103081/00214 ECL 02.00 FPGA-Vs=AF
     6   0x26 0x19   0x8    AE  S  2.0 SGU-3  AQS SGU/2 600 Z103081/00169 ECL 02.00 FPGA-Vs=AF
    21   0x21 0xcf     0        P  0.0 PSD-1  PSD/3 Power Supply Distribution Board
    --   0x20 0xc6     0        B  1.2 AQS/2  AQS/2 chassis
     1   0x20  0x7     0        B      MASTER AQS Rack Master
  Logical Receiver/SGU configuration:


Router: none installed


Transmitters at the spectrometer subnet:
----------------------------------------
BLA_W1345092_0044 W1345092/0044 ECL 0:
- TCP/IP address = 149.236.99.254
- Firmware VS    = 20120627
- Amplifier      = BLAX300 E 6-365MHZ: W1345092/0044 ECL 0
- Router         = BLMMR31 RF AMPLIFIER MODULE: W1345212/0143 ECL 0
- Controller     = BLA CONTROL BOARD 6 1V V-USB: W1522041/0116 ECL 1
BLA_W1345096_0069 W1345096/0069 ECL 1:
- TCP/IP address = 149.236.99.253
- Firmware VS    = 20120627
- Amplifier      = BLAXH2H300/100/150 E 200-600MHZ: W1345096/0069 ECL 1
- Router         = BLMMR32 RF AMPLIFIER MODULE: W1345204/0065 ECL 0
- Controller     = BLA CONTROL BOARD 6 2V V-USB: W1522040/0268 ECL 1
- QNP-Accessory  : 1 X-input and 1 H-input

BSMS: BSMS/2 connected to ethernet
- TCP/IP address = 149.236.99.20
- ELCB firmware version = 20130627
- GAB current limits = 0.0/X, 0.0/Y, 10.0/Z (in A)
- SCB channels = 40
- Shim System = BOSS2-SB
- 2HTX Amplifier: not available
- Lock: installed

Bruker Automatic Changer: device connected to 149.236.99.249:/dev/tty04
- Capacity: 24 holders
- Firmware: 970111
- use BACS air  = yes
- BACS sx delay = 10 s
- Sample Rail fast changer mode = no

Eurotherm VTU: device connected to 149.236.99.249:/dev/tty05

Preamplifiers :
HPPR: - HPPR/2 preamplifier connected to 149.236.99.89:/dev/tty10
    Type      : HPPR/2
    Controller: Application firmware = AQ
                15 LEDs for tuning, 15 LEDs for matching
    Module  1 : 1H LNA
                 PN=Z003462, SN=00471 from 20060828
    Module  2 : XBB19F 2HS
                 PN=Z003506, SN=00512 from 20060914
    Module  3 : XBB19F 2HS
                 PN=Z003506, SN=00513 from 20060914
    Module  4 : 2H
                 PN=Z003473, SN=00473 from 20060913


Frequency generation:
- F1: for SGU
- F2: for SGU
- F3: for SGU



RF cable connections (detected by 'confamp')
--------------------------------------------------------------------
SGU1 NORM output -> input 1 of transmitter 2 (BLAXH2H300/100/150 E 200-600MHZ W1345096/0069 at TCP/IP 149.236.99.253)
SGU1 AUX  output -> input 2 of transmitter 1 (BLAX300 E 6-365MHZ W1345092/0044 at TCP/IP 149.236.99.254)
SGU2 NORM output -> input 2 of transmitter 2 (BLAXH2H300/100/150 E 200-600MHZ W1345096/0069 at TCP/IP 149.236.99.253)
SGU2 AUX  output -> TUNE signal input of HPPR
SGU3 NORM output -> input 1 of transmitter 1 (BLAX300 E 6-365MHZ W1345092/0044 at TCP/IP 149.236.99.254)
SGU3 AUX  output -> input 4 of transmitter 2 (BLAXH2H300/100/150 E 200-600MHZ W1345096/0069 at TCP/IP 149.236.99.253)

Blanking cable connections (detected by 'confamp')
--------------------------------------------------------------------
transmitter 1 (BLAX300 E 6-365MHZ W1345092/0044 at TCP/IP 149.236.99.254) amplifier X-300W uses blanking 4
transmitter 2 (BLAXH2H300/100/150 E 200-600MHZ W1345096/0069 at TCP/IP 149.236.99.253) amplifier 1H-100W uses blanking 2
transmitter 2 (BLAXH2H300/100/150 E 200-600MHZ W1345096/0069 at TCP/IP 149.236.99.253) amplifier X-300W uses blanking 1
transmitter 2 (BLAXH2H300/100/150 E 200-600MHZ W1345096/0069 at TCP/IP 149.236.99.253) amplifier 2H-150W needs no blanking

Switchbox (3 outputs: X / F / H) routing
--------------------------------------------------------------------
BLAXH2H300/100/150 E 200-600MHZ W1345096/0069 at TCP/IP 149.236.99.253 amplifier X-300W at blanking 1 can be routed to switchbox output 1 = X and output 2 = F
BLAXH2H300/100/150 E 200-600MHZ W1345096/0069 at TCP/IP 149.236.99.253 amplifier 1H-100W at blanking 2 can be routed to switchbox output 1 = X, output 2 = F and output 3 = H
BLAXH2H300/100/150 E 200-600MHZ W1345096/0069 at TCP/IP 149.236.99.253 amplifier 2H-150W can be routed to switchbox output 5 (unknown)

